









1. Turn on the printer and connect the USB to the computer, and then open the small ticket driver installation program  
   
2. Select language (currently only Chinese and English are supported)  
   
3. Select the installation file path (this step is best to keep the default and not modify it, which is convenient for later maintenance)  
   
4. Select additional tasks (it is recommended to check (create icons on the desktop) for this step to facilitate later maintenance)  
   
5. Click install  
   
6. Run Nomal POS Driver after installation  
   
7. Select the printer model according to the printing width of the small ticket machine (MP POS 58 MM/MP POS 80 MM)  
   
8. After selecting the printer model, confirm that the printer is turned on and the USB is connected to the computer, click the "USB port detection" button  
   
9. After the program detects the USB port, click the "install driver" button  
   
10. After waiting for a period of time, the computer will automatically pop up the printer properties of the installed driver  
    
11. 点击打印测试页，如打印机出纸，则打印机已经安装完成